# Commands:

Before reading, note that the commands are NOT case sensitive, “shw m” should work just as well as i.e.: “sHW m”;

Displaying information:

- *SHW S:*

Display mother-ship information;

- *SHW D* [drone id]:

Display selected drone information;

- *SHW M:*

Display local map;

Resource gathering:

- *MINE S:*

Mine the object the mother-ship is currently on;

- *MINE D* [drone id]:

Mine the object the selected drone is currently on;

- *COL D* [drone id]:

Return the selected drone to the mother-ship and collect its resources;

Navigation:

- *NAV S* [x] [y]:

Navigate the mother-ship to the specified x and y coordinates. Note that x and y values < 10 must be written with 2 numbers, i.e.: 0 = 00; 1 = 01…;

- *NAV D* [drone id] [x] [y]:

Navigate the selected drone to the specified x and y coordinates. Note that x and y values < 10 must be written with 2 numbers, i.e.: 0 = 00; 1 = 01…;

Component Control:

- *A C* [component id]:

Activate selected component;

- *D C* [component id]:

Deactivate selected component;

- *U C* [component id]:

Upgrade selected component;

- *B C* [component name]:

Build specified component.